**Excitation LED Printed Circuit Board Fabrication Information**

* Number of layers: 2
* Substrate: 0.031” FR4
* Board width: 5mm
* Board height: 7.5mm
* Copper weight: 1oz (not important)
* Surface: HASL or ENIG (not important)
* Board shape: Custom
* Cutouts: None
* Solder mask color: Black
* Sinkscreen layers: Bottom
* Sinkscreen color: White
* Electrical Test: Not required
* Routing: Either individual or panalized with v-scores